,Model##other##,Description##other##,Volts##other##,Cycle##other##,Phase##other##,FL Amps##other##,Max Overcurrent Protection##other##,Watts##other##,Electric Connection Type##other##,Conn Plug##other##,Conn Conduit##other##,Weight in Pounds##other##
,,,,,,,,,,,,
High Speed Combination Oven,,,,,,,,,,,,
,,,,,,,,,,,,
JET514A (230/1/50),JET514A,High Speed Combination Oven,230,50,1,13,15,2900,,Type 1 Australia,0,112
,,,,,,,,,,,,
JET514C (220/1/50),JET514C,High Speed Combination Oven,220,50,1,13,16,2900,,China 3-Pin Angle Type,0,112
,,,,,,,,,,,,
JET514VC (220/1/50),JET514VC,High Speed Combination Oven,220,50,1,13,16,2900,,China 3-Pin Angle Type,0,112
,,,,,,,,,,,,
JET514I (230/1/50),JET514I,High Speed Combination Oven,230,50,1,13,16,2900,,BS546,0,112
,,,,,,,,,,,,
JET14K (220/1/60),JET14K,High Speed Combination Oven,220,60,1,16,16,3200,,KS Approved Type F,0,112
,,,,,,,,,,,,
JET14VK (220/1/60),JET14VK,High Speed Combination Oven,220,60,1,16,16,3200,,KS Approved Type F,0,112
,,,,,,,,,,,,
JET14VT (380/3/60),JET14VT,High Speed Combination Oven,380,60,3,16,16,3300,Direct Wire,,1,112
